*** Creating Trace Output File 'GPIOint.tra' Ok.
### Preparing for ADS-LD.
### Creating ADS-LD Command Line
### List of Objects: adding '"lpc2300.o"'
### List of Objects: adding '"gpioint.o"'
### List of Objects: adding '"lcd_4bit.o"'
### ADS-LD Command completed:
"lpc2300.o" "gpioint.o" "lcd_4bit.o" --device DARMP --strict --scatter "GPIOint.sct" 

--autoat --summary_stderr --info summarysizes --map --xref --callgraph --symbols 

--info sizes --info totals --info unused --info veneers 

 --list ".\GPIOint.map" -o "GPIOint.axf"### Preparing Environment (PrepEnvAds)
### ADS-LD Output File: 'GPIOint.axf'
### ADS-LD Command File: 'GPIOint.lnp'
### Checking for dirty Components...
### Creating CmdFile 'GPIOint.lnp', Handle=0x0000011C
### Writing '.lnp' file
### ADS-LD Command file 'GPIOint.lnp' is ready.
### ADS-LD: About to start ADS-LD Thread.
### ADS-LD: executed with 0 errors
### Updating obj list
### LDADS_file() completed.
